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Navigation Notice No 1 of 2023
Berthing/Unberthing operation in the port of San Nicolas
Following a procedural review, there have been a number of observations regarding berthing operations at certain terminals located in the port of San Nicolas, namely “Puerto Nuevo”, “Central Térmica” and “Grain Elevator” (“The Terminals”)
The roads and maneuvering areas within the port limits of San Nicolas are narrow, and there is almost no current nearby the Terminals, altogether making the berthing and unberthing operation more challenging. Nevertheless, the employment of tugs is not compulsory for berthing nor unberthing as per local authority. Hence, the procedure relies mainly on the vessel´s power, ropes handling and the use of the anchor. 
Notwithstanding the lack of regulations regarding the use of tugs, the Harbour Pilots of the Parana River recommends the use of tugs at the Terminals referred above, in any of the the following circumstances:
1) When the vessel’s draught is equal or deeper than 8,50 meters, regardless of her length overall.

2) When the vessel’s length overall is equal or greater than 178 meters regardless of her draught. 

3) In case of unfavorable hydrometeorogical conditions.

Should the hydrometeorological conditions are unfavorable, and the master decides not to appoint tugs, the berthing/unberthing operation may be delayed, and will depend on the judgement of the boarding Pilot taking into account the improvements of the weather condition.
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Descripción generada automáticamente]Owners, Agents, Operators should ensure that the contents of this Navigation Notice are made known to the Masters of their vessels. 
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Aviso de Navegación No 1 de 2023
Operación de atraque/ Zarpada en el puerto de San Nicolás

Luego de una revisión de procedimientos, se han realizado una serie de observaciones con respecto a las operaciones de atraque en ciertas terminales ubicadas en el puerto de San Nicolás, a saber, “Puerto Nuevo”, “Central Térmica” y “Elevador de Granos” (“Las Terminales”).
[bookmark: _GoBack]
Las zonas de maniobra dentro de los límites del puerto de San Nicolás son estrechas y la corriente en el área de las Terminales es prácticamente nula, lo cual incrementa el grado de dificultad en las maniobras. No obstante, el uso de remolcadores no es obligatorio según la autoridad local tanto para las maniobras de amarre o desamarre. Por lo tanto, el procedimiento depende principalmente de la máquina del buque, del manipuleo de los cabos de amarre y del uso del ancla.

Sin perjuicio de la falta de reglamentación, los Prácticos de Puerto del Río Paraná recomiendan el uso de remolcadores en las Terminales antes referidas, en cualquiera las siguientes circunstancias:

1) Cuando el calado del buque sea igual o superior a 8,50 metros, cualquiera que sea su eslora total.

2) Cuando la eslora total del buque sea igual o superior a 178 metros cualquiera que sea su calado.

3) Cuando las condiciones hidrometeorológicas sean desfavorables.

En caso de que las condiciones hidrometeorológicas sean desfavorables y el capitán decida no utilizar remolcadores, la operación de atraque/desatraque podrá demorarse y dependerá del criterio del Práctico que embarque teniendo en consideración las mejoras en las condiciones presentes.

Los Propietarios, Agentes, Operadores deben asegurarse de que el contenido de este Aviso de Navegación sea conocido por los Capitanes de sus buques.
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Marcelo Ledesma
                                                                                                                  Presidente






APPENDIX 1


[image: ]



[image: ]
image1.png




image2.png




image3.png




image4.png
NG

qumad‘

Isla de
Cattaneo

&P ecolde san)

& Ic:l}é:de
2% los Aifoyos
J { o Puertolingeniero
] 1 /Club'SOMISAY =
/ JJfiSector de\peé'ca‘\A' o Buitrago
SIS 4 (i S MuellelCarbon Siderar
L (i TS
4% % \





image5.png
BOSQUES

(20MT)

A QUMICA

N

%[2 _.

Srpaia

QUMICA

* [LaMT)
il
TERMINAL
GBNNCOLAS £ EvaDOR DE

(22MT) BEMTUGRLAS "
4 @ . Toug? (AR
@

VADORRDE
NOS@RN Ni

o QSIL o5 28MT) (7oMT)
MS)

(it

CENTRAL

TERMOELEGH RI
™ MR ARMICTY -- asMT)




